	
		EDIT AND PERFORM SCANVUE REBOOT

5/12/11


The following instruction:
   ModeSet -r xx.xx.xx.xx
(where xx.xx.xx.xx is ScanVue IP address) is used to reboot individual ScanVue units.

REBOOT.BAT may be used to reboot multiple ScanVue units sequentially.

NOTE: An application for performing timed auto-reboot is not available from IEE
for customer use. However, ModeSet or REBOOT.BAT files may be inserted into a
custom application to perform timed auto-reboot as needed.


EDITING--------------------------------------------------
1) To edit batch program REBOOT.BAT using Notepad or other editor.
   Right click REBOOT.BAT and choose Edit.
2) Modify IP addresses as needed for ScanVue units to be rebooted and save REBOOT.BAT.


REBOOT---------------------------------------------------
1) Make sure ModeSet.exe and REBOOT.BAT files are placed in the same directory.
2) Double click edited program REBOOT.BAT and verify ScanVue units reboot.
